|  |  |
| --- | --- |
| Coin-Operated Breath Alcohol TesterAlcolab is a coin-operated breath alcohol tester that can be used in public places like bars, restaurants, or any place where alcohol is consumed. It provides law-enforcement accuracy and a user-friendly operation for users to administer their own alcohol tests with convenience and confidence. | |
| **Taking a Breath Test** | |
|  | 1. When the ***1 Insert coins*** message is lit up, Alcolab is ready for a test. 2. Insert the required number of coins into the coin slot on the side. 3. The ***2 Place STRAW in port message*** lights up. 4. Take a straw from the bottom and insert it into the sampling port.   *Note. Do not drink or smoke at least 20 minutes prior to the test.*   1. When **3 Blow Steadily until tone ends** lights up, blow into the straw moderately and continuously for approximately 5 seconds. You should hear a tone that indicates a proper breath flow.   *Note. If you blow too hard, too soft or intermittently, Alcolab may be unable to collect a proper breath sample and the tone will stop. Blow again and make sure that a continuous tone is heard.*   1. Stop blowing when the tone stops and you hear a beep. 2. You will see a **Please Wait…** message as Alcolab analyzes the result.   *Note. The average time taken to analyze the result is between 5-10 seconds and varies based on the level of alcohol present.*   1. The result is shown in **Your level** window and the legal limit is displayed in the **Limit** window above it. 2. Depending on your alcohol content, one of these indicators light up: **Be careful - Don’t drive** or **Over the limit**. If no alcohol is detected, the **No alcohol detected** indicator lights up. 3. **Please wait** message flashes again as Alcolab prepares for another test.   *Note: Depending on the alcohol content of the previous test, there may be a delay of up to 30 seconds. The* ***1 Insert coins*** *message lights up when Alcolab is ready for the next test.* |